E-Z-GO RXV Chameleon Installation Instructions
1.	Remove the enclosure, club protector, tracks, and hardware from the box and lay it out so you can familiarize yourself with the different pieces.

2.	Remove the windshield from your cart. Completely unzip and remove the sleeve portion of the front door of the enclosure.  Wrap the sleeve around the windshield frame so that the cut out for the windshield retention clip is toward the top end of the sleeve (the sleeves are side specific so make sure they are put on the correct side). Engage the smaller zipper so that it wraps snugly around the windshield frame. The zipper should be on the backside of the windshield frame.  Adjust the height of the sleeve as necessary for even alignment after the sides are installed and zipped to the sleeves.  See Picture 1.

3.	Note:  The side tracks should be installed with the bead pointing down and to the outside of the cart.  The front edge of the enclosure should line up with the windshield frame.  The cold curtain track should be installed with the bead pointing down and to the inside of the cart.

4.	Install the rear track by aligning the ends of the rail with the edge of the rear canopy strut pocket.  Center the rail and drill the outside hole using a 5/32" bit.  Attach with 2 screws.  Mark and drill the center hole and install screw.  See Picture 2.  Install the cold curtain onto the rail.  

5.	Side tracks:  Drill four 5/32 holes in the long track, two holes 2 inches in from the ends and two holes 15 inches from each end.  Zip the curtains on one side together and the zip them to the front sleeve.  Slide the aluminum track onto the curtains using the bottom channel with the bead pointing down and to the outside of the cart and the cutout portion toward the front top support.  The track should be centered between the top metal supports. With the curtains hanging properly, attach it to the top using the self-drilling screws provided.  The bottom flap of the back section of the side curtains tuck under the seat.  Repeat for the opposite side.  See photo 3 & 4.

6.	Install the valance in the top channel.  Install the plastic caps in each end of the valance channel to keep the valance in place.   With the enclosure totally zipped together and hanging properly pinch each end of the tracks that the curtains are in to keep them from sliding.

7.	Attach the bottom center section of the ultra seal cold curtain (closeout panel) to each end section and to the seat back using the Velcro strips.  See Picture 5.

8.	If your enclosure has body snaps install the male portion of the snaps on the body of the cart using the pop rivets provided.  The enclosure should be snug but not to tight.

9.	Re-installing your windshield:  If using a support bolt for the windshield, cut a small “X” in the sleeve to allow for placement of the support bolt through the windshield frame and sleeve.  Un-zip the sleeve to expose the back side of the windshield frame where the support bolt hole is.  Reverse the bolt by inserting it from the backside of the windshield frame.  Attach the windshield by carefully snapping the windshield extrusion around the sleeve and frame.  Attach the nut to the supporting bolt and tighten.  Re-zip the sleeve.

Club Protector Installation:

1.	Remove rear most nuts and bolts from bag hoop assembly.  Retain hardware.  
2.	Attach bottom bag cover bar using hardware removed in step #1.  See Picture 6.  
3.	Center the awning rail between the rear canopy struts.  Use rail as a guide to mark and drill 5/32” holes.  Attach rail using 3 screws.  See Picture 7.  
4.	Slide bag cover into rail.  See picture 8.  
5.	Attach cover to bottom bar using pins.  See Picture 9.